

Maroondah PLANNING SCHEME

[bookmark: _GoBack]*Given the pending translation of the Maroondah Planning Scheme into the MPS/PPF format by Smart Planning in response to VC148, this policy is provided as a supporting document to show the likely translated format of the Clause 22.15 ESD policy.
15.02-1L	Environmentally sustainable development--/--/--- 
C---

	Policy application
This policy applies to residential and non-residential development, excluding subdivisions in accordance with the thresholds detailed in this Policy.
	Objective
To achieve best practice in environmentally sustainable development from the design stage through to construction and operation.
	Strategies
Facilitate development that minimises environmental impacts.
Encourage environmentally sustainable development that:
· Is consistent with the type and scale of the development.
· Responds to site opportunities and constraints.
· Uses a combination of methods, processes and locally available technology that demonstrably minimise environmental impacts.
	Energy performance
Reduce both energy use and energy peak demand through design measures such as:
· Building orientation.
· Shading to glazed surfaces.
· Optimising glazing to exposed surfaces.
· Inclusion of or space allocation for renewable technologies.
	Integrated water management
Reduce total operating potable water use through appropriate design measures such as water efficient fixtures, appliances, equipment, irrigation and landscaping.
Encourage the appropriate use of alternative water sources (including greywater, rainwater and stormwater).
Incorporate best practice water sensitive urban design to improve the quality of stormwater runoff and reduce impacts on water systems and water bodies.
	Indoor environment quality
Achieve a healthy indoor environment quality, including thermal performance and access to fresh air and daylight, prioritising passive design over mechanical heating, ventilation, cooling and lighting.
Reduce indoor air pollutants by encouraging use of non-toxic materials.
Minimise noise levels and noise transfer within and between buildings and associated external areas.
	Transport
Design development to promote the use of walking, cycling and public transport, in that order; and minimise car dependency.
Promote the use of low emissions vehicle technologies and supporting infrastructure.
	Waste management
Promote waste avoidance, reuse and recycling during the design, construction and operation stages of development.
Encourage use of durable and reusable building materials.
Ensure sufficient space is allocated for future change in waste management needs, including (where possible) composting and green waste facilities.
	Urban ecology
Protect and enhance biodiversity by incorporating natural habitats and planting indigenous vegetation.
Reduce urban heat island effects through building design, landscape design, water sensitive urban design and the retention and provision of canopy and significant trees.
Encourage the provision of space for productive gardens, particularly in larger residential developments.
	Policy guidelines
Residential and mixed use development with a residential component
A Sustainable Design Assessment (including an assessment using BESS, STORM or other methods) for:
· 3 - 9 dwellings; or
· Alterations and additions creating 500 square metres or more of additional gross floor space (excluding outbuildings).
A Sustainability Management Plan (including an assessment using BESS, STORM, Green star, MUSIC or other methods) and a Green Travel Plan for:
· 10 or more dwellings; or
· A building used for accommodation (other than a dwelling) with a gross floor area of more than 1,000 square metres; or
· Alterations and additions creating 1,000 square metres or more of additional gross floor space.
Non-residential
A Sustainable Design Assessment (including an assessment using BESS, STORM, MUSIC or other methods) and a Green Travel Plan for:
· A non-residential building with a gross floor area of 500 square metres and 999 square metres; or
· Alterations and additions creating between 500 square metres and 999 square metres of additional gross floor area.
A Sustainability Management Plan (including an assessment using BESS, STORM, Green star, MUSIC or other methods) and a Green Travel Plan for:
· A non-residential building with a gross floor area of more than 1,000 square metres; or
· Alterations and additions creating more than 1,000 square metres of additional gross floor area.
Consider as relevant the following tools to support a Sustainable Design Assessment or Sustainable Management Plan:
· Sustainable Design Assessment in the Planning Process (IMAP, 2015)
· Built Environment Sustainability Scorecard ‘BESS’ (Council Alliance for a Sustainable Built Environment ‘CASBE’, 2015)
· Green Star (Green Building Council of Australia)
· Model for Urban Stormwater Improvement Conceptualisation ‘MUSIC’ (Melbourne Water)
· Nationwide House Energy Rating Scheme ‘NatHERS’ (Department of Climate Change and Energy Efficiency)
· Stormwater Treatment Objective - Relative Measure ‘STORM’ (Melbourne Water)
· Urban Stormwater Best Practice Environmental Management Guidelines (Victorian Stormwater Committee, 1999)
· Waste Management and Recycling in Multi-Unit Developments - Better Practice Guide (Sustainability Victoria, 2018).
	Expiry
This policy will expire if it is superseded by a comparable provision of the Victoria Planning Provisions.


OFFICIAL

