MAROONDAH PLANNING SCHEME
	SCHEDULE 5 TO CLAUSE 32.09 NEIGHBOURHOOD RESIDENTIAL ZONE--/--/2018
C116

Shown on the planning scheme map as NRZ5.
	JUBILEE PARK
1.0	Neighbourhood character objectives--/--/2018
C116

To ensure that the spacious and modest residential character of Jubilee Park is respected and enhanced.
To ensure low scale building forms, consistent with the neighbourhood character of the area.
To ensure that all dwellings, their settings and front fences make a positive contribution to the public domain and pedestrian environment.
To maintain a sense of spaciousness around dwellings, when viewed from the street.
To ensure that front setbacks are not dominated by garages, carports or vehicular access.

2.0	Minimum subdivision area--/--/2018
C116


None specified

3.0	Permit requirement for the construction or extension of one dwelling or a fence associated with a dwelling on a lot--/--/2018
C116


	
	Requirement 

	Permit requirement for the construction or extension of one dwelling on a lot
	None specified


	Permit requirement to construct or extend a front fence within 3 metres of a street associated with a dwelling on a lot
	None specified



4.0	Requirements of Clause 54 and Clause 55--/--/2018
C116


	
	Standard
	Requirement

	Minimum street setback
	A3 and B6
	None specified

	Site coverage
	A5 and B8
	None specified

	Permeability
	A6 and B9
	None specified

	Landscaping
	B13
	None specified

	Side and rear setbacks
	A10 and B17
	Side setbacks
1.2 metres, plus 0.3 metres for every metre of height over 3.6 metres up to 6.9 metres, plus 1 metre for every metre of height over 6.9 metres.
Rear setbacks
5 metres, plus 0.3 metres for every metre of height over 3.6 metres up to 6.9 metres, plus 1 metre for every metre of height over 6.9 metres.

	Walls on boundaries
	A11 and B18
	None specified

	Private open space
	A17 
	An area of 80 square metres, with one part of the private open space to consist of secluded private open space at the side or rear of the dwelling with a minimum area of  60 square metres, a minimum dimension of 5 metres and convenient access from a living room.

	
	B28
	An area of 80 square metres, with one part of the private open space to consist of secluded private open space at the side or rear of the dwelling with a minimum area of  60 square metres, a minimum dimension of 5 metres and convenient access from a living room.


	Front fence height
	A20 and B32
	0.9 metres


5.0	Maximum building height requirement for a dwelling or residential building--/--/2018
C116


None specified
6.0	Application requirements--/--/2018
C116


None specified
7.0	Decision guidelines--/--/2018
[bookmark: _GoBack]C116


The following decision guidelines apply to an application for a permit under Clause 32.09, in addition to those specified in Clause 32.09 and elsewhere in the scheme which must be considered, as appropriate, by the responsible authority:

 The extent to which the proposed buildings or works meet the neighbourhood character objectives of this clause.
The extent to which any building to be demolished, extended or otherwise modified, contributes to the preferred neighbourhood character of the area. 
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